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Plant pre-use check
Blank sheet for a week of daily pre-use checks on one item of plant, with weekly checks and a fault log.
Keep plant maintained in efficient working order and good repair. If it has a maintenance log, keep the log up to date.
Inspect plant that is exposed to conditions causing deterioration at suitable intervals, and after anything that could affect its safety. Record the result and keep it until the next inspection is recorded.
Decide what to check, and how often, from your risk assessment and the manufacturer's instructions. Simple pre-use checks do not normally need to be recorded. Use this sheet if you want a record of them.
Plant used for lifting also needs a thorough examination by a competent person at least every 12 months, or every 6 months if it lifts people, unless an examination scheme sets other intervals.
The plant
	Type of plant
	
	Make, model and fleet or serial number
	

	Owner or hire company
	
	Site
	

	Operator
	
	Week beginning
	

	Last service date
	
	Next thorough examination due (lifting equipment)
	



Daily pre-use checks
Do the manufacturer's daily checks. Tick each item that is in order, and report any fault so it can be put right before it becomes a risk.
	Check
	Mon
	Tue
	Wed
	Thu
	Fri
	Sat
	Sun

	Manufacturer's daily checks done
	
	
	
	
	
	
	

	Brakes work
	
	
	
	
	
	
	

	Lights work
	
	
	
	
	
	
	

	Controls work
	
	
	
	
	
	
	

	Seat belt or other restraint in good order
	
	
	
	
	
	
	

	Mirrors and CCTV give a clear view
	
	
	
	
	
	
	

	Checked by (initials)
	
	
	
	
	
	
	



Weekly checks
Typical weekly checks include guards, safety devices, tyre pressures, and the condition of windows, mirrors and CCTV on mobile plant.
	Check
	Date
	In order
	Notes

	Guards in place
	
	
	

	Safety devices work
	
	
	

	Tyres and tyre pressures
	
	
	

	Windows, mirrors and CCTV in good condition
	
	
	

	Rollover protection (ROPS) undamaged, where fitted
	
	
	



Faults reported
	Date
	Fault
	Reported to
	Taken out of use?
	Put right (date and by whom)

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	



Based on: The Provision and Use of Work Equipment Regulations 1998 (PUWER), regulations 5 and 6; HSE, Inspection of work equipment and Mobile work equipment; the Lifting Operations and Lifting Equipment Regulations 1998 (LOLER), regulation 9; HSE, Thorough examinations and inspections of lifting equipment.
Provision and Use of Work Equipment Regulations 1998, regulation 5: https://www.legislation.gov.uk/uksi/1998/2306/regulation/5
Provision and Use of Work Equipment Regulations 1998, regulation 6: https://www.legislation.gov.uk/uksi/1998/2306/regulation/6
HSE, Inspection of work equipment: https://www.hse.gov.uk/work-equipment-machinery/inspection.htm
HSE, Mobile work equipment: https://www.hse.gov.uk/work-equipment-machinery/mobile.htm
Lifting Operations and Lifting Equipment Regulations 1998, regulation 9: https://www.legislation.gov.uk/uksi/1998/2307/regulation/9
HSE, Thorough examinations and inspections of lifting equipment: https://www.hse.gov.uk/work-equipment-machinery/thorough-examinations-lifting-equipment.htm
Blank template from The Site Book, October 2026. Fill it in for the actual job and site.
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